Kajima BASIC Pump Commands


In order to run the Kajima Basic Program that controls the pump PLC via the RS-422/485 link, perform the following steps:

1. Hook up the PLC RS-422/485 Interface cable to COM2 of the desired PC.

2. Run the Command Prompt from the Start Menu/Accessories

3. Switch to the right directory containing GWBASIC.EXE by using the cd (change directory) DOS command.

4. Then, type gwbasic followed by <Enter> key.

5. After gwbasic starts, type:

load “pctoplc.asc”<Enter>

run<Enter>

The pump control program should start displaying the send/receive data.

The following single character commands are used with the pump control command.  Each time a character is entered, a “3005” will be printed to indicate that a key command has been received.  Some of the commands will also print a message to tell the user what command was just issued.

The proper sequence is to shut off the pilot pumps with a PLC E-STOP (Pilot OFF does exactly the same thing).  ALWAYS start the system with an E-STOP followed by a RESET.

The keyboard caps lock CANNOT be on.  The characters must be lower case.

Kajima BASIC Pump Commands

The following commands are used:

Character

Function


e

PLC E-STOP


r

PLC RESET


p

Pilot Pressure ON/OFF (toggles)


l

Low Pressure ON/OFF (toggles)


h

High Pressure ON/OFF (toggles)

0-8 Selects number of pumps 0-8 to be used for low/high pressure

s

Display known bits

a

Static Lift Solenoid A ON/OFF (toggles)

b

Static Lift Solenoid B ON/OFF (toggles)

c

Static Lift Solenoid C ON/OFF (toggles)

d

Static Lift Solenoid D ON/OFF (toggles)

x

Charge Static Lift ON/OFF (toggles)

y

Dump Static Lift ON/OFF (toggles)

q

Charge Blow-Down (toggles)

z

Enable Blow-Down (toggles)
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